
Notice of compliance form
Rentals 
Minnesota Statutes 327.32, Subd. 1 (c) 
This notice must be completed and signed by the renter(s) and the landlord(s) of the used manufactured home described in the purchase agreement and at the bottom of this notice before the parties transfer ownership of a used manufactured home constructed after June 14, 1976.
Manufactured Home Installation System Seal Number	
Renter’s name(s)	
Landlord’s name(s)	

Smoke alarms are installed and operational in accordance with the Code of Federal Regulations, Title 24, section 3280.209, or are installed in each bedroom and outside of bedrooms in the vicinity of bedroom doors. The center of smoke detectors shall be located within 12 inches of the ceiling. Alarms are less than 10 years old and will be less than 10 years old at the end of a lease agreement. The manufacture date is printed on the back.
Verification (check one, then each party initial):  	Complies    	Correction Required	  Renter: 	Lessor:	
Carbon monoxide alarms or carbon monoxide detectors are approved, operational and are installed within 10 feet of each room lawfully used for sleeping purposes.
Verification (check one, then each party initial):  	Complies    	Correction Required	  Renter: 	Lessor:	
Egress windows are in every bedroom with at least one openable window with a net clear opening of 20 inches wide and 24 inches high, five square feet in area, with the bottom of window openings no more than 36 inches above the floor. Locks, latches, operating handles, tabs, or other operational devices are located not more than 54 inches above the finished floor.
Verification (check one, then each party initial):  	Complies   Correction Required	  Renter: 	Lessor:	
Electric range and clothes dryer have electrical outlets that accept plugs with four prongs.
Verification (check one, then each party initial): 	 Complies    Correction Required	  Renter: 	Lessor:	
The domestic water heater is listed for manufactured home use under the Code of Federal Regulations, Title 24, section 3280.709(a) and (d)(1) and (2), and installed correctly in accordance with federal standards.
Verification (check one, then each party initial):  	Complies    	Correction Required	  Renter: 	Lessor:	
The water heater enclosure is completed with an interior finish of gypsum board, vinyl coated gypsum board panels or other materials having a flame spread rating not exceeding 25.
Verification (check one, then each party initial):  	Complies    	Correction Required	  Renter: 	Lessor:	
The furnace is listed for manufactured home use under the Code of Federal Regulations, title 24, section 3280.709(a) and (d)(1) and (2), and installed correctly in accordance with federal standards.
Verification (check one, then each party initial):  	Complies    	Correction Required	  Renter: 	Lessor:	
The furnace enclosure is completed with an interior finish of gypsum board, vinyl-coated gypsum board panels, or other materials having a flame spread rating not exceeding 25.
Verification (check one, then each party initial):  	Complies    	Correction Required	  Renter: 	Lessor:	
Solid fuel burning fireplaces or stoves are listed for use in manufactured homes under the Code of Federal Regulations, title 24, section 3280.709(g), and installed correctly in accordance with the federal regulations, including chimney, doors, hearth, combustion or intake.
Verification (check one, then each party initial):  	Complies    	Correction Required	  Renter: 	Lessor:	
The home complies with code requirements for snow load and heat zone requirements as indicated by the data plate.
Verification (check one, then each party initial):  	Complies    	Correction Required	  Renter: 	Lessor:	
Correction activities require construction permits from the local building official or from the state of Minnesota, and inspections are required to verify compliance with corrections.
The parties to this agreement have initialed all required sections and agree by their signature that all items listed comply prior to the tenant's occupancy of the home described below, as listed in the lease agreement. The state of Minnesota or a local building official has the authority to inspect the home in the manner described in Minnesota Statutes, section 327.33, prior to or after occupancy to ensure compliance was properly executed as provided under the Manufactured Home Building Code.  
Signatures of the renter(s)
Printed name as appears on the rental agreement	Signature	Date
		
		

Signatures of the landlord(s)
Printed name and license number, if applicable	Signature	Date
		
		



Home information
Street address of home at time of sale		
City, state, ZIP code	
Name of home manufacturer	
Model of home, and year constructed	
Serial number	
Installation label number	
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